---- printf Matches (130 in 10 files) ----
AD5318_Ctrl in AD5318.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //    printf("ShiftTarget : %x \r\n",ShiftTarget);
N_Divider_Reg_Create in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("FRAC : %d INT : %d \r\n",(int)_FRAC,_INT);
N_Divider_Reg_Create in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\nLINE : %d  ret : %x\r\n",__LINE__,ret);
N_Divider_Reg_Create in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\nLINE : %d  ret : %x\r\n",__LINE__,ret);    
N_Divider_Reg_Create in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\nLINE : %d  ret : %x\r\n",__LINE__,ret);    
N_Divider_Reg_Create in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\nLINE : %d  ret : %x\r\n",__LINE__,ret);
R_Divider_Reg_Create in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("_MOD : %d INT : %d \r\n",_MOD,_RCOUNTER);
R_Divider_Reg_Create in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\nLINE : %d  ret : %x\r\n",__LINE__,ret);
R_Divider_Reg_Create in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\nLINE : %d  ret : %x\r\n",__LINE__,ret);
ADF4153_Freq_Calc in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\ntemp_adf4153.N_Value : %f  temp_adf4153.INT_Value : %f  temp_adf4153.MOD_Value : %f \r\n",temp_adf4153.N_Value,(double)temp_adf4153.INT_Value,(double)temp_adf4153.MOD_Value);
ADF4153_Freq_Calc in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\n temp_adf4153.N_Value - (double)temp_adf4153.INT_Value) : %f  temp * (double)temp_adf4153.MOD_Value : %f \r\n",temp,temp * (double)temp_adf4153.MOD_Value);
ADF4153_Freq_Calc in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\ntemp_adf4153.N_Value : %x   : %f ",temp_adf4153.N_Value,((double)(Freq / 1000) /  (double)(temp_adf4153.PFD_Value / 1000)) / 1000);
ADF4153_Freq_Calc in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("temp_adf4153.MOD_Value : %x   : %d \r\n",temp_adf4153.MOD_Value,temp_adf4153.MOD_Value);
ADF4153_Freq_Calc in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("1");
ADF4153_Freq_Calc in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("0");
ADF4153_Freq_Calc in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\n");
ADF4153_Freq_Calc in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("temp_adf4153.FRAC_Value : %x   : %d\r\n",temp_adf4153.FRAC_Value,temp_adf4153.FRAC_Value);
ADF4153_Freq_Calc in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("1");
ADF4153_Freq_Calc in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("0");
ADF4153_Freq_Calc in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\n");    
ADF4153_Freq_Calc in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("temp_adf4153.INT_Value : %x   : %d\r\n",temp_adf4153.INT_Value,temp_adf4153.INT_Value); 
ADF4153_Freq_Calc in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("1");
ADF4153_Freq_Calc in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("0");
ADF4153_Freq_Calc in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\n");    
ADF4153_Freq_Calc in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("R0: %x  R1: %x \r\n",N_Divider_Reg_Create(temp_adf4153.FRAC_Value,temp_adf4153.INT_Value,0),R_Divider_Reg_Create(temp_adf4153.MOD_Value,R_Counter,1,0,2,0));   
ADF4153_Initialize in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :         printf("\r\nPLL_EN_3_5G_H_GPIO_Port\r\n");
ADF4153_Module_Ctrl in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("YJ :R0: %x  R1:  %x   R2 : %x R3 : %x ",R0,R1,R2,R3);
ADF4153_Module_Ctrl in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\n");
ADF4153_Module_Ctrl in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("1");
ADF4153_Module_Ctrl in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("0");
ADF4153_Module_Ctrl in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\n");
ADF4153_Module_Ctrl in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :              printf("1");
ADF4153_Module_Ctrl in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :              printf("0");
ADF4153_Module_Ctrl in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :      printf("\r\n");
ADF4153_Module_Ctrl in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("1");
ADF4153_Module_Ctrl in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("0");
ADF4153_Module_Ctrl in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\n");
ADF4153_Module_Ctrl in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("1");
ADF4153_Module_Ctrl in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("0");
ADF4153_Module_Ctrl in adf4153.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\n");
BDA4601_atten_ctrl in BDA4601.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //    printf("BDA4601_atten_ctrl : %x \r\n",data);
BDA4601_atten_ctrl in BDA4601.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //                     printf("1");
BDA4601_atten_ctrl in BDA4601.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //                printf("0");
Jump_App in flash.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("boot loader start\n");               //硫붿꽭占�? 異쒕젰
Jump_App in flash.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("jump!\n");
Flash_InitRead in flash.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :         printf("%08x : %02X \n",Address ,*(uint8_t*)Address);
Flash_InitRead in flash.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :         printf("%08x : %02X \n",Address ,*(uint8_t*)Address);
Flash_InitRead in flash.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :         printf("%02X ",*(uint8_t*)Address);
Flash_RGB_Data_Write in flash.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("HAL NOT OK \n");
Flash_write in flash.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("Erase Failed \r\n");
FLASH_Byte_Write in flash.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //  printf("Flash Write Start \r\n");
FLASH_Byte_Write in flash.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("Eraser Error\r\n");
FLASH_Byte_Write in flash.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("Write Error %d\r\n",__LINE__);
FLASH_Byte_Write in flash.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("Addr = %x, Data = %x\r\n", FLASH_USER_START_ADDR + i, *(__IO uint16_t *)(FLASH_USER_START_ADDR + i));
Bluecell_Flash_Read in flash.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("Addr = %x, Data = %x\r\n", FLASH_USER_START_ADDR + i, *(__IO uint16_t *)(FLASH_USER_START_ADDR + i));
Bluecell_Flash_Read in flash.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :         printf("Data = %x\r\n",  data[i]);
kConstPrinter in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("%s", Bluecell_Prot_IndexStr[k]);
Power_ON_OFF_Ctrl in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //    printf("\r\ntype : %s cmd : %d\r\n",Bluecell_Prot_IndexStr[type - 4],cmd);
Power_ON_OFF_Ctrl in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("\r\n LINE %d\r\n",__LINE__);
Power_ON_OFF_Ctrl in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("\r\n LINE %d\r\n",__LINE__);
Power_ON_OFF_Ctrl in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("\r\n LINE %d\r\n",__LINE__);
Power_ON_OFF_Ctrl in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("\r\n LINE %d\r\n",__LINE__);
Power_ON_OFF_Ctrl in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //                printf("\r\n LINE %d\r\n",__LINE__);
Power_ON_OFF_Ctrl in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //                printf("\r\n LINE %d\r\n",__LINE__);
Power_ON_OFF_Ctrl in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //                            printf("\r\n LINE %d\r\n",__LINE__);
Power_ON_OFF_Ctrl in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //                            printf("\r\n LINE %d\r\n",__LINE__);
Power_ON_OFF_Ctrl in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("\r\n LINE %d\r\n",__LINE__);
Power_ON_OFF_Ctrl in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("\r\n LINE %d\r\n",__LINE__);
Power_ON_OFF_Ctrl in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //            printf("\r\n LINE %d\r\n",__LINE__);
Power_ON_OFF_Ctrl in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //            printf("\r\n LINE %d\r\n",__LINE__);
Power_ON_OFF_Ctrl in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("TDD SYNC OPERATE ; %d\r\n",cmd);
Power_ON_OFF_Ctrl in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :         printf("Function : %s LINE : %d   ERROR \r\n",__func__,__LINE__);
ATTEN_PLL_PATH_Initialize in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("Data = %x\r\n",  Flash_Save_data[i]);
ADC_Check in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :           printf("Prev_data[%d] : %x",i,Prev_data[INDEX_DET_1_8G_DL_IN_H + i]);
ADC_Check in includes.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :           printf("%x\r\n",i,Prev_data[INDEX_DET_1_8G_DL_IN_L + i]);            
assert_failed in main.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :      tex: printf("Wrong parameters value: file %s on line %d\r\n", file, line) */
PE43711_ALL_atten_ctrl in PE43711.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //    printf("why not? \r\n");
halSynSetFreq in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("FREQ:%f Mhz  B : %d , A  : %d    N_VAL  : %d \r\n",(float)(rf_Freq/1000000),B,A,N_val);
halSynSetFreq in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("YJ 4113 : %x \r\n",N_Counter_Latch_Create(A,B,0));
N_Counter_Latch_Create in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("_ACOUNTER : %d _BCOUNTER : %d \r\n",_ACOUNTER,_BCOUNTER);
N_Counter_Latch_Create in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\nLINE : %d  ret : %x\r\n",__LINE__,ret);
N_Counter_Latch_Create in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\nLINE : %d  ret : %x\r\n",__LINE__,ret);
N_Counter_Latch_Create in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\nLINE : %d  ret : %x\r\n",__LINE__,ret);
N_Counter_Latch_Create in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\nLINE : %d  ret : %x\r\n",__LINE__,ret);
N_Counter_Latch_Create in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("\r\nLINE : %d  ret : %x\r\n",__LINE__,ret);
ADF4113_Module_Ctrl in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("1");
ADF4113_Module_Ctrl in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("0");
ADF4113_Module_Ctrl in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :      printf("\r\n");
ADF4113_Module_Ctrl in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("1");
ADF4113_Module_Ctrl in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("0");
ADF4113_Module_Ctrl in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :         printf("\r\n");
ADF4113_Module_Ctrl in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("1");
ADF4113_Module_Ctrl in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("0");            
ADF4113_Module_Ctrl in pll_4113.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :         printf("\r\n");
HAL_UART_RxCpltCallback in uart.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //    printf("Function : %s : \r\n",__func__);
GetDataFromUartQueue in uart.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("%02x ",*(pQueue->Buffer + pQueue->tail)) ;
GetDataFromUartQueue in uart.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("data cnt zero !!!  \r\n");
GetDataFromUartQueue in uart.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :                 printf("%02x ",uart_buf[i]);
RF_Data_Check in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("Recv CRC Value : \"%d\"\r\n Create CRC Value : \"%d\"   \r\n",data_buf[data_buf[Crcindex]],STH30_CreateCrc(&data_buf[Type], data_buf[Length]));
RF_Data_Check in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //    printf("CRC Result : \"%d\"   \r\n",ret);
RF_Status_Get in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //    printf("\r\nYJ2 : Prev_data[INDEX_DET_1_8G_DL_IN_L ] : %x\r\n",Prev_data[INDEX_DET_1_8G_DL_IN_L]);            
RF_Status_Get in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //    printf("\r\nYJ : %x",ADCvalue[0]);
RF_Status_Get in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //    printf("\r\n");
RF_Status_Ack in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //    printf("\r\nYJ2 : Prev_data[INDEX_DET_1_8G_DL_IN_L ] : %x\r\n",Prev_data[INDEX_DET_1_8G_DL_IN_L]);            
RF_Status_Ack in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //    printf("\r\nYJ : %x",ADCvalue[0]);
RF_Status_Ack in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //    printf("\r\n");
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //    printf("Prev_data[INDEX_ATT_1_8G_DL1]  : %x  data_buf[INDEX_ATT_1_8G_DL1] : %x\r\n",Prev_data[INDEX_ATT_1_8G_DL1],data_buf[INDEX_ATT_1_8G_DL1]);
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("data_buf[INDEX_PLL_1_8G_DL_H] : %x \r\n",data_buf[INDEX_PLL_1_8G_DL_H]);
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("data_buf[INDEX_PLL_1_8G_DL_L] : %x\r\n",data_buf[INDEX_PLL_1_8G_DL_L]);
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("data_buf[INDEX_PLL_1_8G_UL_H] : %x \r\n",data_buf[INDEX_PLL_1_8G_UL_H]);
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("data_buf[INDEX_PLL_1_8G_UL_L] : %x\r\n",data_buf[INDEX_PLL_1_8G_UL_L]);
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("data_buf[INDEX_PLL_2_1G_DL_H] : %x \r\n",data_buf[INDEX_PLL_2_1G_DL_H]);
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("data_buf[INDEX_PLL_2_1G_DL_L] : %x\r\n",data_buf[INDEX_PLL_2_1G_DL_L]);
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("data_buf[INDEX_PLL_2_1G_UL_H] : %x \r\n",data_buf[INDEX_PLL_2_1G_UL_H]);
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("data_buf[INDEX_PLL_2_1G_UL_L] : %x\r\n",data_buf[INDEX_PLL_2_1G_UL_L]);
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("POWER : %d \r\n",Prev_data[INDEX_PLL_ON_OFF_3_5G_H]);
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //            printf("PLL CTRL START !! \r\n");
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("POWER : %d \r\n",Prev_data[INDEX_PLL_ON_OFF_3_5G_L]);        
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //            printf("PLL CTRL START !! \r\n");
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("Prev_data[INDEX_DAC_VCtrl_C_H] : %x \r\n",Prev_data[INDEX_DAC_VCtrl_C_H]);
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("Prev_data[INDEX_DAC_VCtrl_C_L] : %x \r\n",Prev_data[INDEX_DAC_VCtrl_C_L]);
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("DAC CTRL START \r\n");
RF_Operate in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("DAC Change\r\n");
RF_Ctrl_Main in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("%02x ",data_buf[i]);
RF_Ctrl_Main in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :         printf("Reset Start \r\n");
RF_Ctrl_Main in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :     printf("TYPE_BLUECELL_SET : ");
RF_Ctrl_Main in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :         printf("%02x ",data_buf[i]);
RF_Ctrl_Main in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :         printf("\r\nTYPE_BLUECELL_GET : \r\n");
RF_Ctrl_Main in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : //        printf("\r\nFLASH Write\r\n");
RF_Ctrl_Main in zig_operate.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             printf("Function : %s   LINE : %d    type : %d \r\n",__func__,__LINE__,type);
