---- HAL_Delay Matches (14 in 6 files) ----
EEPROM_M24C08_Read in eeprom.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :             HAL_Delay(20);
EEPROM_M24C08_write in eeprom.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :                 HAL_Delay(20);
EEPROM_M24C08_write in eeprom.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :                 HAL_Delay(20);
EEPROM_M24C08_write in eeprom.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :                  HAL_Delay(20);
EEPROM_M24C08_write in eeprom.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :              HAL_Delay(20);
EEPROM_M24C08_Zerowrite in eeprom.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :              HAL_Delay(20);
Flash_RGB_Data_Write in flash.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :       //  HAL_Delay(1);
main in main.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) : 	  //HAL_Delay(500);
stm32f1xx_hal.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Drivers\STM32F1xx_HAL_Driver\Src) line 131 :              time intervals. Care must be taken if HAL_Delay() is called from a
stm32f1xx_hal.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Drivers\STM32F1xx_HAL_Driver\Src) line 153 :   * @note   SysTick is used as time base for the HAL_Delay() function, the application
stm32f1xx_hal.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Drivers\STM32F1xx_HAL_Driver\Src) line 242 :   *       Care must be taken if HAL_Delay() is called from a peripheral ISR process,
stm32f1xx_hal.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Drivers\STM32F1xx_HAL_Driver\Src) line 374 : __weak void HAL_Delay(uint32_t Delay)
stm32f1xx_hal.h (D:\workspace\STM32F103_ATTEN_PLL_Zig\Drivers\STM32F1xx_HAL_Driver\Inc) line 312 : void HAL_Delay(uint32_t Delay);
GetDataFromUartQueue in uart.c (D:\workspace\STM32F103_ATTEN_PLL_Zig\Src) :        // HAL_Delay(1);
