---- HAL_UART Matches (600 in 9 files) ----
Uart_Data_Send in atten_ctrl.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     HAL_UART_Transmit_DMA(&huart3, data,size);
_write in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     HAL_UART_Transmit (&huart1, ptr, len, 10);
main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) line 142 : void HAL_UART_RxCpltCallback(UART_HandleTypeDef *huart)
HAL_UART_RxCpltCallback in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :         HAL_UART_Receive_DMA(&huart3,&rx2_data,1);
main in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     HAL_UART_Receive_DMA(&huart3, &rx2_data,1);
MX_USART1_UART_Init in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :   if (HAL_UART_Init(&huart1) != HAL_OK)
MX_USART3_UART_Init in main.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :   if (HAL_UART_Init(&huart3) != HAL_OK)
stm32f2xx_hal_conf.h (D:\workspace\STM32F207_ChannelCtrlProject\Inc) line 59 : #define HAL_UART_MODULE_ENABLED
stm32f2xx_hal_conf.h (D:\workspace\STM32F207_ChannelCtrlProject\Inc) line 164 : #define  USE_HAL_UART_REGISTER_CALLBACKS        0U /* UART register callback disabled      */
stm32f2xx_hal_conf.h (D:\workspace\STM32F207_ChannelCtrlProject\Inc) line 355 : #ifdef HAL_UART_MODULE_ENABLED
stm32f2xx_hal_conf.h (D:\workspace\STM32F207_ChannelCtrlProject\Inc) line 356 :  #include "stm32f2xx_hal_uart.h"
stm32f2xx_hal_conf.h (D:\workspace\STM32F207_ChannelCtrlProject\Inc) line 357 : #endif /* HAL_UART_MODULE_ENABLED */
stm32f2xx_hal_msp.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) line 235 : void HAL_UART_MspInit(UART_HandleTypeDef* huart)
stm32f2xx_hal_msp.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) line 369 : void HAL_UART_MspDeInit(UART_HandleTypeDef* huart)
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 3 :   * @file    stm32f2xx_hal_uart.c
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 20 :     (#) Initialize the UART low level resources by implementing the HAL_UART_MspInit() API:
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 25 :         (##) NVIC configuration if you need to use interrupt process (HAL_UART_Transmit_IT()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 26 :              and HAL_UART_Receive_IT() APIs):
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 29 :         (##) DMA Configuration if you need to use DMA process (HAL_UART_Transmit_DMA()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 30 :              and HAL_UART_Receive_DMA() APIs):
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 46 :         the HAL_UART_Init() API.
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 59 :             __HAL_UART_ENABLE_IT() and __HAL_UART_DISABLE_IT() inside the transmit
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 63 :        (@) These APIs (HAL_UART_Init() and HAL_HalfDuplex_Init()) configure also the
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 65 :             HAL_UART_MspInit() API.
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 71 :     The compilation define USE_HAL_UART_REGISTER_CALLBACKS when set to 1
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 75 :     Use Function @ref HAL_UART_RegisterCallback() to register a user callback.
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 76 :     Function @ref HAL_UART_RegisterCallback() allows to register following callbacks:
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 91 :     Use function @ref HAL_UART_UnRegisterCallback() to reset a callback to the default
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 93 :     @ref HAL_UART_UnRegisterCallback() takes as parameters the HAL peripheral handle,
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 108 :     By default, after the @ref HAL_UART_Init() and when the state is HAL_UART_STATE_RESET
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 110 :     examples @ref HAL_UART_TxCpltCallback(), @ref HAL_UART_RxHalfCpltCallback().
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 112 :     reset to the legacy weak (surcharged) functions in the @ref HAL_UART_Init()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 113 :     and @ref HAL_UART_DeInit() only when these callbacks are null (not registered beforehand).
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 114 :     If not, MspInit or MspDeInit are not null, the @ref HAL_UART_Init() and @ref HAL_UART_DeInit()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 118 :     Callbacks can be registered/unregistered in HAL_UART_STATE_READY state only.
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 120 :     in HAL_UART_STATE_READY or HAL_UART_STATE_RESET state, thus registered (user)
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 123 :     using @ref HAL_UART_RegisterCallback() before calling @ref HAL_UART_DeInit()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 124 :     or @ref HAL_UART_Init() function.
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 127 :     When The compilation define USE_HAL_UART_REGISTER_CALLBACKS is set to 0 or
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 137 :        (+) Send an amount of data in blocking mode using HAL_UART_Transmit()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 138 :        (+) Receive an amount of data in blocking mode using HAL_UART_Receive()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 143 :        (+) Send an amount of data in non blocking mode using HAL_UART_Transmit_IT()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 144 :        (+) At transmission end of transfer HAL_UART_TxCpltCallback is executed and user can
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 145 :             add his own code by customization of function pointer HAL_UART_TxCpltCallback
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 146 :        (+) Receive an amount of data in non blocking mode using HAL_UART_Receive_IT()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 147 :        (+) At reception end of transfer HAL_UART_RxCpltCallback is executed and user can
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 148 :             add his own code by customization of function pointer HAL_UART_RxCpltCallback
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 149 :        (+) In case of transfer Error, HAL_UART_ErrorCallback() function is executed and user can
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 150 :             add his own code by customization of function pointer HAL_UART_ErrorCallback
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 155 :        (+) Send an amount of data in non blocking mode (DMA) using HAL_UART_Transmit_DMA()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 156 :        (+) At transmission end of half transfer HAL_UART_TxHalfCpltCallback is executed and user can
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 157 :             add his own code by customization of function pointer HAL_UART_TxHalfCpltCallback
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 158 :        (+) At transmission end of transfer HAL_UART_TxCpltCallback is executed and user can
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 159 :             add his own code by customization of function pointer HAL_UART_TxCpltCallback
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 160 :        (+) Receive an amount of data in non blocking mode (DMA) using HAL_UART_Receive_DMA()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 161 :        (+) At reception end of half transfer HAL_UART_RxHalfCpltCallback is executed and user can
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 162 :             add his own code by customization of function pointer HAL_UART_RxHalfCpltCallback
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 163 :        (+) At reception end of transfer HAL_UART_RxCpltCallback is executed and user can
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 164 :             add his own code by customization of function pointer HAL_UART_RxCpltCallback
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 165 :        (+) In case of transfer Error, HAL_UART_ErrorCallback() function is executed and user can
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 166 :             add his own code by customization of function pointer HAL_UART_ErrorCallback
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 167 :        (+) Pause the DMA Transfer using HAL_UART_DMAPause()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 168 :        (+) Resume the DMA Transfer using HAL_UART_DMAResume()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 169 :        (+) Stop the DMA Transfer using HAL_UART_DMAStop()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 176 :       (+) __HAL_UART_ENABLE: Enable the UART peripheral
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 177 :       (+) __HAL_UART_DISABLE: Disable the UART peripheral
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 178 :       (+) __HAL_UART_GET_FLAG : Check whether the specified UART flag is set or not
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 179 :       (+) __HAL_UART_CLEAR_FLAG : Clear the specified UART pending flag
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 180 :       (+) __HAL_UART_ENABLE_IT: Enable the specified UART interrupt
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 181 :       (+) __HAL_UART_DISABLE_IT: Disable the specified UART interrupt
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 182 :       (+) __HAL_UART_GET_IT_SOURCE: Check whether the specified UART interrupt has occurred or not
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 229 : #ifdef HAL_UART_MODULE_ENABLED
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 246 : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 248 : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 298 :     The HAL_UART_Init(), HAL_HalfDuplex_Init(), HAL_LIN_Init() and HAL_MultiProcessor_Init() APIs
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 313 : HAL_StatusTypeDef HAL_UART_Init(UART_HandleTypeDef *huart)
HAL_UART_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if (huart->gState == HAL_UART_STATE_RESET)
HAL_UART_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
HAL_UART_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       huart->MspInitCallback = HAL_UART_MspInit;
HAL_UART_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     HAL_UART_MspInit(huart);
HAL_UART_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* (USE_HAL_UART_REGISTER_CALLBACKS) */
HAL_UART_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_BUSY;
HAL_UART_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   __HAL_UART_DISABLE(huart);
HAL_UART_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   __HAL_UART_ENABLE(huart);
HAL_UART_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->ErrorCode = HAL_UART_ERROR_NONE;
HAL_UART_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_READY;
HAL_UART_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->RxState = HAL_UART_STATE_READY;
HAL_HalfDuplex_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if (huart->gState == HAL_UART_STATE_RESET)
HAL_HalfDuplex_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
HAL_HalfDuplex_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       huart->MspInitCallback = HAL_UART_MspInit;
HAL_HalfDuplex_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     HAL_UART_MspInit(huart);
HAL_HalfDuplex_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* (USE_HAL_UART_REGISTER_CALLBACKS) */
HAL_HalfDuplex_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_BUSY;
HAL_HalfDuplex_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   __HAL_UART_DISABLE(huart);
HAL_HalfDuplex_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   __HAL_UART_ENABLE(huart);
HAL_HalfDuplex_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->ErrorCode = HAL_UART_ERROR_NONE;
HAL_HalfDuplex_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_READY;
HAL_HalfDuplex_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->RxState = HAL_UART_STATE_READY;
HAL_LIN_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if (huart->gState == HAL_UART_STATE_RESET)
HAL_LIN_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
HAL_LIN_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       huart->MspInitCallback = HAL_UART_MspInit;
HAL_LIN_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     HAL_UART_MspInit(huart);
HAL_LIN_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* (USE_HAL_UART_REGISTER_CALLBACKS) */
HAL_LIN_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_BUSY;
HAL_LIN_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   __HAL_UART_DISABLE(huart);
HAL_LIN_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   __HAL_UART_ENABLE(huart);
HAL_LIN_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->ErrorCode = HAL_UART_ERROR_NONE;
HAL_LIN_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_READY;
HAL_LIN_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->RxState = HAL_UART_STATE_READY;
HAL_MultiProcessor_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if (huart->gState == HAL_UART_STATE_RESET)
HAL_MultiProcessor_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
HAL_MultiProcessor_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       huart->MspInitCallback = HAL_UART_MspInit;
HAL_MultiProcessor_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     HAL_UART_MspInit(huart);
HAL_MultiProcessor_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* (USE_HAL_UART_REGISTER_CALLBACKS) */
HAL_MultiProcessor_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_BUSY;
HAL_MultiProcessor_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   __HAL_UART_DISABLE(huart);
HAL_MultiProcessor_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   __HAL_UART_ENABLE(huart);
HAL_MultiProcessor_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->ErrorCode = HAL_UART_ERROR_NONE;
HAL_MultiProcessor_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_READY;
HAL_MultiProcessor_Init in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->RxState = HAL_UART_STATE_READY;
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 619 : HAL_StatusTypeDef HAL_UART_DeInit(UART_HandleTypeDef *huart)
HAL_UART_DeInit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_BUSY;
HAL_UART_DeInit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   __HAL_UART_DISABLE(huart);
HAL_UART_DeInit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
HAL_UART_DeInit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->MspDeInitCallback = HAL_UART_MspDeInit;
HAL_UART_DeInit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   HAL_UART_MspDeInit(huart);
HAL_UART_DeInit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* (USE_HAL_UART_REGISTER_CALLBACKS) */
HAL_UART_DeInit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->ErrorCode = HAL_UART_ERROR_NONE;
HAL_UART_DeInit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_RESET;
HAL_UART_DeInit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->RxState = HAL_UART_STATE_RESET;
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 663 : __weak void HAL_UART_MspInit(UART_HandleTypeDef *huart)
HAL_UART_MspInit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :            the HAL_UART_MspInit could be implemented in the user file
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 678 : __weak void HAL_UART_MspDeInit(UART_HandleTypeDef *huart)
HAL_UART_MspDeInit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :            the HAL_UART_MspDeInit could be implemented in the user file
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 687 : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 694 :   *           @arg @ref HAL_UART_TX_HALFCOMPLETE_CB_ID Tx Half Complete Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 695 :   *           @arg @ref HAL_UART_TX_COMPLETE_CB_ID Tx Complete Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 696 :   *           @arg @ref HAL_UART_RX_HALFCOMPLETE_CB_ID Rx Half Complete Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 697 :   *           @arg @ref HAL_UART_RX_COMPLETE_CB_ID Rx Complete Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 698 :   *           @arg @ref HAL_UART_ERROR_CB_ID Error Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 699 :   *           @arg @ref HAL_UART_ABORT_COMPLETE_CB_ID Abort Complete Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 700 :   *           @arg @ref HAL_UART_ABORT_TRANSMIT_COMPLETE_CB_ID Abort Transmit Complete Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 701 :   *           @arg @ref HAL_UART_ABORT_RECEIVE_COMPLETE_CB_ID Abort Receive Complete Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 702 :   *           @arg @ref HAL_UART_MSPINIT_CB_ID MspInit Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 703 :   *           @arg @ref HAL_UART_MSPDEINIT_CB_ID MspDeInit Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 707 : HAL_StatusTypeDef HAL_UART_RegisterCallback(UART_HandleTypeDef *huart, HAL_UART_CallbackIDTypeDef CallbackID, pUART_CallbackTypeDef pCallback)
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->ErrorCode |= HAL_UART_ERROR_INVALID_CALLBACK;
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if (huart->gState == HAL_UART_STATE_READY)
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_TX_HALFCOMPLETE_CB_ID :
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_TX_COMPLETE_CB_ID :
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_RX_HALFCOMPLETE_CB_ID :
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_RX_COMPLETE_CB_ID :
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_ERROR_CB_ID :
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_ABORT_COMPLETE_CB_ID :
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_ABORT_TRANSMIT_COMPLETE_CB_ID :
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_ABORT_RECEIVE_COMPLETE_CB_ID :
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_MSPINIT_CB_ID :
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_MSPDEINIT_CB_ID :
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->ErrorCode |= HAL_UART_ERROR_INVALID_CALLBACK;
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   else if (huart->gState == HAL_UART_STATE_RESET)
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_MSPINIT_CB_ID :
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_MSPDEINIT_CB_ID :
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->ErrorCode |= HAL_UART_ERROR_INVALID_CALLBACK;
HAL_UART_RegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->ErrorCode |= HAL_UART_ERROR_INVALID_CALLBACK;
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 816 :   *           @arg @ref HAL_UART_TX_HALFCOMPLETE_CB_ID Tx Half Complete Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 817 :   *           @arg @ref HAL_UART_TX_COMPLETE_CB_ID Tx Complete Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 818 :   *           @arg @ref HAL_UART_RX_HALFCOMPLETE_CB_ID Rx Half Complete Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 819 :   *           @arg @ref HAL_UART_RX_COMPLETE_CB_ID Rx Complete Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 820 :   *           @arg @ref HAL_UART_ERROR_CB_ID Error Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 821 :   *           @arg @ref HAL_UART_ABORT_COMPLETE_CB_ID Abort Complete Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 822 :   *           @arg @ref HAL_UART_ABORT_TRANSMIT_COMPLETE_CB_ID Abort Transmit Complete Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 823 :   *           @arg @ref HAL_UART_ABORT_RECEIVE_COMPLETE_CB_ID Abort Receive Complete Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 824 :   *           @arg @ref HAL_UART_MSPINIT_CB_ID MspInit Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 825 :   *           @arg @ref HAL_UART_MSPDEINIT_CB_ID MspDeInit Callback ID
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 828 : HAL_StatusTypeDef HAL_UART_UnRegisterCallback(UART_HandleTypeDef *huart, HAL_UART_CallbackIDTypeDef CallbackID)
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if (HAL_UART_STATE_READY == huart->gState)
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_TX_HALFCOMPLETE_CB_ID :
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->TxHalfCpltCallback = HAL_UART_TxHalfCpltCallback;               /* Legacy weak  TxHalfCpltCallback       */
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_TX_COMPLETE_CB_ID :
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->TxCpltCallback = HAL_UART_TxCpltCallback;                       /* Legacy weak TxCpltCallback            */
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_RX_HALFCOMPLETE_CB_ID :
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->RxHalfCpltCallback = HAL_UART_RxHalfCpltCallback;               /* Legacy weak RxHalfCpltCallback        */
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_RX_COMPLETE_CB_ID :
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->RxCpltCallback = HAL_UART_RxCpltCallback;                       /* Legacy weak RxCpltCallback            */
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_ERROR_CB_ID :
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->ErrorCallback = HAL_UART_ErrorCallback;                         /* Legacy weak ErrorCallback             */
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_ABORT_COMPLETE_CB_ID :
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->AbortCpltCallback = HAL_UART_AbortCpltCallback;                 /* Legacy weak AbortCpltCallback         */
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_ABORT_TRANSMIT_COMPLETE_CB_ID :
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->AbortTransmitCpltCallback = HAL_UART_AbortTransmitCpltCallback; /* Legacy weak AbortTransmitCpltCallback */
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_ABORT_RECEIVE_COMPLETE_CB_ID :
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->AbortReceiveCpltCallback = HAL_UART_AbortReceiveCpltCallback;   /* Legacy weak AbortReceiveCpltCallback  */
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_MSPINIT_CB_ID :
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->MspInitCallback = HAL_UART_MspInit;                             /* Legacy weak MspInitCallback           */
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_MSPDEINIT_CB_ID :
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->MspDeInitCallback = HAL_UART_MspDeInit;                         /* Legacy weak MspDeInitCallback         */
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->ErrorCode |= HAL_UART_ERROR_INVALID_CALLBACK;
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   else if (HAL_UART_STATE_RESET == huart->gState)
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_MSPINIT_CB_ID :
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->MspInitCallback = HAL_UART_MspInit;
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       case HAL_UART_MSPDEINIT_CB_ID :
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->MspDeInitCallback = HAL_UART_MspDeInit;
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->ErrorCode |= HAL_UART_ERROR_INVALID_CALLBACK;
HAL_UART_UnRegisterCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->ErrorCode |= HAL_UART_ERROR_INVALID_CALLBACK;
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 923 : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 948 :            The HAL_UART_TxCpltCallback(), HAL_UART_RxCpltCallback() user callbacks
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 950 :            The HAL_UART_ErrorCallback()user callback will be executed when a communication error is detected.
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 953 :         (+) HAL_UART_Transmit()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 954 :         (+) HAL_UART_Receive()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 957 :         (+) HAL_UART_Transmit_IT()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 958 :         (+) HAL_UART_Receive_IT()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 959 :         (+) HAL_UART_IRQHandler()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 962 :         (+) HAL_UART_Transmit_DMA()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 963 :         (+) HAL_UART_Receive_DMA()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 964 :         (+) HAL_UART_DMAPause()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 965 :         (+) HAL_UART_DMAResume()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 966 :         (+) HAL_UART_DMAStop()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 969 :         (+) HAL_UART_TxHalfCpltCallback()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 970 :         (+) HAL_UART_TxCpltCallback()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 971 :         (+) HAL_UART_RxHalfCpltCallback()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 972 :         (+) HAL_UART_RxCpltCallback()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 973 :         (+) HAL_UART_ErrorCallback()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 976 :         (+) HAL_UART_Abort()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 977 :         (+) HAL_UART_AbortTransmit()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 978 :         (+) HAL_UART_AbortReceive()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 979 :         (+) HAL_UART_Abort_IT()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 980 :         (+) HAL_UART_AbortTransmit_IT()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 981 :         (+) HAL_UART_AbortReceive_IT()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 983 :     (#) For Abort services based on interrupts (HAL_UART_Abortxxx_IT), a set of Abort Complete Callbacks are provided:
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 984 :         (+) HAL_UART_AbortCpltCallback()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 985 :         (+) HAL_UART_AbortTransmitCpltCallback()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 986 :         (+) HAL_UART_AbortReceiveCpltCallback()
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 993 :            and HAL_UART_ErrorCallback() user callback is executed. Transfer is kept ongoing on UART side.
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 997 :            Error code is set to allow user to identify error type, and HAL_UART_ErrorCallback() user callback is executed.
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 1000 :         and receive process in parallel, the UART state HAL_UART_STATE_BUSY_TX_RX can't be useful.
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 1018 : HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout)
HAL_UART_Transmit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if (huart->gState == HAL_UART_STATE_READY)
HAL_UART_Transmit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->ErrorCode = HAL_UART_ERROR_NONE;
HAL_UART_Transmit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->gState = HAL_UART_STATE_BUSY_TX;
HAL_UART_Transmit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->gState = HAL_UART_STATE_READY;
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 1103 : HAL_StatusTypeDef HAL_UART_Receive(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout)
HAL_UART_Receive in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if (huart->RxState == HAL_UART_STATE_READY)
HAL_UART_Receive in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->ErrorCode = HAL_UART_ERROR_NONE;
HAL_UART_Receive in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->RxState = HAL_UART_STATE_BUSY_RX;
HAL_UART_Receive in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->RxState = HAL_UART_STATE_READY;
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 1194 : HAL_StatusTypeDef HAL_UART_Transmit_IT(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size)
HAL_UART_Transmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if (huart->gState == HAL_UART_STATE_READY)
HAL_UART_Transmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->ErrorCode = HAL_UART_ERROR_NONE;
HAL_UART_Transmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->gState = HAL_UART_STATE_BUSY_TX;
HAL_UART_Transmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     __HAL_UART_ENABLE_IT(huart, UART_IT_TXE);
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 1239 : HAL_StatusTypeDef HAL_UART_Receive_IT(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size)
HAL_UART_Receive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if (huart->RxState == HAL_UART_STATE_READY)
HAL_UART_Receive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->ErrorCode = HAL_UART_ERROR_NONE;
HAL_UART_Receive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->RxState = HAL_UART_STATE_BUSY_RX;
HAL_UART_Receive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     __HAL_UART_ENABLE_IT(huart, UART_IT_PE);
HAL_UART_Receive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     __HAL_UART_ENABLE_IT(huart, UART_IT_ERR);
HAL_UART_Receive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     __HAL_UART_ENABLE_IT(huart, UART_IT_RXNE);
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 1290 : HAL_StatusTypeDef HAL_UART_Transmit_DMA(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size)
HAL_UART_Transmit_DMA in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if (huart->gState == HAL_UART_STATE_READY)
HAL_UART_Transmit_DMA in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->ErrorCode = HAL_UART_ERROR_NONE;
HAL_UART_Transmit_DMA in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->gState = HAL_UART_STATE_BUSY_TX;
HAL_UART_Transmit_DMA in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     __HAL_UART_CLEAR_FLAG(huart, UART_FLAG_TC);
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 1358 : HAL_StatusTypeDef HAL_UART_Receive_DMA(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size)
HAL_UART_Receive_DMA in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if (huart->RxState == HAL_UART_STATE_READY)
HAL_UART_Receive_DMA in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->ErrorCode = HAL_UART_ERROR_NONE;
HAL_UART_Receive_DMA in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->RxState = HAL_UART_STATE_BUSY_RX;
HAL_UART_Receive_DMA in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     __HAL_UART_CLEAR_OREFLAG(huart);
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 1425 : HAL_StatusTypeDef HAL_UART_DMAPause(UART_HandleTypeDef *huart)
HAL_UART_DMAPause in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if ((huart->gState == HAL_UART_STATE_BUSY_TX) && dmarequest)
HAL_UART_DMAPause in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if ((huart->RxState == HAL_UART_STATE_BUSY_RX) && dmarequest)
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 1462 : HAL_StatusTypeDef HAL_UART_DMAResume(UART_HandleTypeDef *huart)
HAL_UART_DMAResume in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if (huart->gState == HAL_UART_STATE_BUSY_TX)
HAL_UART_DMAResume in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if (huart->RxState == HAL_UART_STATE_BUSY_RX)
HAL_UART_DMAResume in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     __HAL_UART_CLEAR_OREFLAG(huart);
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 1498 : HAL_StatusTypeDef HAL_UART_DMAStop(UART_HandleTypeDef *huart)
HAL_UART_DMAStop in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :      to call the HAL UART API under callbacks HAL_UART_TxCpltCallback() / HAL_UART_RxCpltCallback():
HAL_UART_DMAStop in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :      and the correspond call back is executed HAL_UART_TxCpltCallback() / HAL_UART_RxCpltCallback()
HAL_UART_DMAStop in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if ((huart->gState == HAL_UART_STATE_BUSY_TX) && dmarequest)
HAL_UART_DMAStop in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if ((huart->RxState == HAL_UART_STATE_BUSY_RX) && dmarequest)
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 1550 : HAL_StatusTypeDef HAL_UART_Abort(UART_HandleTypeDef *huart)
HAL_UART_Abort in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :           huart->ErrorCode = HAL_UART_ERROR_DMA;
HAL_UART_Abort in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :           huart->ErrorCode = HAL_UART_ERROR_DMA;
HAL_UART_Abort in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->ErrorCode = HAL_UART_ERROR_NONE;
HAL_UART_Abort in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->RxState = HAL_UART_STATE_READY;
HAL_UART_Abort in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_READY;
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 1632 : HAL_StatusTypeDef HAL_UART_AbortTransmit(UART_HandleTypeDef *huart)
HAL_UART_AbortTransmit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :           huart->ErrorCode = HAL_UART_ERROR_DMA;
HAL_UART_AbortTransmit in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_READY;
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 1683 : HAL_StatusTypeDef HAL_UART_AbortReceive(UART_HandleTypeDef *huart)
HAL_UART_AbortReceive in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :           huart->ErrorCode = HAL_UART_ERROR_DMA;
HAL_UART_AbortReceive in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->RxState = HAL_UART_STATE_READY;
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 1737 : HAL_StatusTypeDef HAL_UART_Abort_IT(UART_HandleTypeDef *huart)
HAL_UART_Abort_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :          will lead to call HAL_UART_AbortCpltCallback() at end of DMA abort procedure */
HAL_UART_Abort_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :          will lead to call HAL_UART_AbortCpltCallback() at end of DMA abort procedure */
HAL_UART_Abort_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->ErrorCode = HAL_UART_ERROR_NONE;
HAL_UART_Abort_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->gState  = HAL_UART_STATE_READY;
HAL_UART_Abort_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->RxState = HAL_UART_STATE_READY;
HAL_UART_Abort_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
HAL_UART_Abort_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     HAL_UART_AbortCpltCallback(huart);
HAL_UART_Abort_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 1865 : HAL_StatusTypeDef HAL_UART_AbortTransmit_IT(UART_HandleTypeDef *huart)
HAL_UART_AbortTransmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :          will lead to call HAL_UART_AbortCpltCallback() at end of DMA abort procedure */
HAL_UART_AbortTransmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       huart->gState = HAL_UART_STATE_READY;
HAL_UART_AbortTransmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
HAL_UART_AbortTransmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       HAL_UART_AbortTransmitCpltCallback(huart);
HAL_UART_AbortTransmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
HAL_UART_AbortTransmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->gState = HAL_UART_STATE_READY;
HAL_UART_AbortTransmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
HAL_UART_AbortTransmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     HAL_UART_AbortTransmitCpltCallback(huart);
HAL_UART_AbortTransmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 1942 : HAL_StatusTypeDef HAL_UART_AbortReceive_IT(UART_HandleTypeDef *huart)
HAL_UART_AbortReceive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :          will lead to call HAL_UART_AbortCpltCallback() at end of DMA abort procedure */
HAL_UART_AbortReceive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       huart->RxState = HAL_UART_STATE_READY;
HAL_UART_AbortReceive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
HAL_UART_AbortReceive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       HAL_UART_AbortReceiveCpltCallback(huart);
HAL_UART_AbortReceive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
HAL_UART_AbortReceive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->RxState = HAL_UART_STATE_READY;
HAL_UART_AbortReceive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
HAL_UART_AbortReceive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     HAL_UART_AbortReceiveCpltCallback(huart);
HAL_UART_AbortReceive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2012 : void HAL_UART_IRQHandler(UART_HandleTypeDef *huart)
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       huart->ErrorCode |= HAL_UART_ERROR_PE;
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       huart->ErrorCode |= HAL_UART_ERROR_NE;
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       huart->ErrorCode |= HAL_UART_ERROR_FE;
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       huart->ErrorCode |= HAL_UART_ERROR_ORE;
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     if (huart->ErrorCode != HAL_UART_ERROR_NONE)
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       if (((huart->ErrorCode & HAL_UART_ERROR_ORE) != RESET) || dmarequest)
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :                will lead to call HAL_UART_ErrorCallback() at end of DMA abort procedure */
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :             HAL_UART_ErrorCallback(huart);
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :           HAL_UART_ErrorCallback(huart);
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         HAL_UART_ErrorCallback(huart);
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
HAL_UART_IRQHandler in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->ErrorCode = HAL_UART_ERROR_NONE;
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2158 : __weak void HAL_UART_TxCpltCallback(UART_HandleTypeDef *huart)
HAL_UART_TxCpltCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :            the HAL_UART_TxCpltCallback could be implemented in the user file
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2173 : __weak void HAL_UART_TxHalfCpltCallback(UART_HandleTypeDef *huart)
HAL_UART_TxHalfCpltCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :            the HAL_UART_TxHalfCpltCallback could be implemented in the user file
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2188 : __weak void HAL_UART_RxCpltCallback(UART_HandleTypeDef *huart)
HAL_UART_RxCpltCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :            the HAL_UART_RxCpltCallback could be implemented in the user file
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2203 : __weak void HAL_UART_RxHalfCpltCallback(UART_HandleTypeDef *huart)
HAL_UART_RxHalfCpltCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :            the HAL_UART_RxHalfCpltCallback could be implemented in the user file
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2218 : __weak void HAL_UART_ErrorCallback(UART_HandleTypeDef *huart)
HAL_UART_ErrorCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :            the HAL_UART_ErrorCallback could be implemented in the user file
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2232 : __weak void HAL_UART_AbortCpltCallback(UART_HandleTypeDef *huart)
HAL_UART_AbortCpltCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :             the HAL_UART_AbortCpltCallback can be implemented in the user file.
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2247 : __weak void HAL_UART_AbortTransmitCpltCallback(UART_HandleTypeDef *huart)
HAL_UART_AbortTransmitCpltCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :             the HAL_UART_AbortTransmitCpltCallback can be implemented in the user file.
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2262 : __weak void HAL_UART_AbortReceiveCpltCallback(UART_HandleTypeDef *huart)
HAL_UART_AbortReceiveCpltCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :             the HAL_UART_AbortReceiveCpltCallback can be implemented in the user file.
HAL_LIN_SendBreak in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_BUSY;
HAL_LIN_SendBreak in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_READY;
HAL_MultiProcessor_EnterMuteMode in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_BUSY;
HAL_MultiProcessor_EnterMuteMode in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_READY;
HAL_MultiProcessor_ExitMuteMode in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_BUSY;
HAL_MultiProcessor_ExitMuteMode in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_READY;
HAL_HalfDuplex_EnableTransmitter in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_BUSY;
HAL_HalfDuplex_EnableTransmitter in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_READY;
HAL_HalfDuplex_EnableReceiver in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_BUSY;
HAL_HalfDuplex_EnableReceiver in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_READY;
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2461 :    (+) HAL_UART_GetState() API can be helpful to check in run-time the state of the UART peripheral.
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2462 :    (+) HAL_UART_GetError() check in run-time errors that could be occurred during communication.
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2474 : HAL_UART_StateTypeDef HAL_UART_GetState(UART_HandleTypeDef *huart)
HAL_UART_GetState in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   return (HAL_UART_StateTypeDef)(temp1 | temp2);
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2489 : uint32_t HAL_UART_GetError(UART_HandleTypeDef *huart)
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2511 : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
UART_InitCallbacksToDefault in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->TxHalfCpltCallback        = HAL_UART_TxHalfCpltCallback;        /* Legacy weak TxHalfCpltCallback        */
UART_InitCallbacksToDefault in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->TxCpltCallback            = HAL_UART_TxCpltCallback;            /* Legacy weak TxCpltCallback            */
UART_InitCallbacksToDefault in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->RxHalfCpltCallback        = HAL_UART_RxHalfCpltCallback;        /* Legacy weak RxHalfCpltCallback        */
UART_InitCallbacksToDefault in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->RxCpltCallback            = HAL_UART_RxCpltCallback;            /* Legacy weak RxCpltCallback            */
UART_InitCallbacksToDefault in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->ErrorCallback             = HAL_UART_ErrorCallback;             /* Legacy weak ErrorCallback             */
UART_InitCallbacksToDefault in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->AbortCpltCallback         = HAL_UART_AbortCpltCallback;         /* Legacy weak AbortCpltCallback         */
UART_InitCallbacksToDefault in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->AbortTransmitCpltCallback = HAL_UART_AbortTransmitCpltCallback; /* Legacy weak AbortTransmitCpltCallback */
UART_InitCallbacksToDefault in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->AbortReceiveCpltCallback  = HAL_UART_AbortReceiveCpltCallback;  /* Legacy weak AbortReceiveCpltCallback  */
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2525 : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
UART_DMATransmitCplt in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
UART_DMATransmitCplt in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     HAL_UART_TxCpltCallback(huart);
UART_DMATransmitCplt in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
UART_DMATxHalfCplt in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
UART_DMATxHalfCplt in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   HAL_UART_TxHalfCpltCallback(huart);
UART_DMATxHalfCplt in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
UART_DMAReceiveCplt in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :     huart->RxState = HAL_UART_STATE_READY;
UART_DMAReceiveCplt in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
UART_DMAReceiveCplt in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   HAL_UART_RxCpltCallback(huart);
UART_DMAReceiveCplt in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
UART_DMARxHalfCplt in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
UART_DMARxHalfCplt in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   HAL_UART_RxHalfCpltCallback(huart);
UART_DMARxHalfCplt in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
UART_DMAError in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if ((huart->gState == HAL_UART_STATE_BUSY_TX) && dmarequest)
UART_DMAError in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if ((huart->RxState == HAL_UART_STATE_BUSY_RX) && dmarequest)
UART_DMAError in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->ErrorCode |= HAL_UART_ERROR_DMA;
UART_DMAError in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
UART_DMAError in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   HAL_UART_ErrorCallback(huart);
UART_DMAError in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
UART_WaitOnFlagUntilTimeout in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   while ((__HAL_UART_GET_FLAG(huart, Flag) ? SET : RESET) == Status)
UART_WaitOnFlagUntilTimeout in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->gState  = HAL_UART_STATE_READY;
UART_WaitOnFlagUntilTimeout in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :         huart->RxState = HAL_UART_STATE_READY;
UART_EndTxTransfer in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_READY;
UART_EndRxTransfer in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->RxState = HAL_UART_STATE_READY;
UART_DMAAbortOnError in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
UART_DMAAbortOnError in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   HAL_UART_ErrorCallback(huart);
UART_DMAAbortOnError in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
UART_DMATxAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->ErrorCode = HAL_UART_ERROR_NONE;
UART_DMATxAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState  = HAL_UART_STATE_READY;
UART_DMATxAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->RxState = HAL_UART_STATE_READY;
UART_DMATxAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
UART_DMATxAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   HAL_UART_AbortCpltCallback(huart);
UART_DMATxAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
UART_DMARxAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->ErrorCode = HAL_UART_ERROR_NONE;
UART_DMARxAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState  = HAL_UART_STATE_READY;
UART_DMARxAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->RxState = HAL_UART_STATE_READY;
UART_DMARxAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
UART_DMARxAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   HAL_UART_AbortCpltCallback(huart);
UART_DMARxAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2851 :   *         HAL_UART_AbortTransmit_IT API (Abort only Tx transfer)
UART_DMATxOnlyAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_READY;
UART_DMATxOnlyAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
UART_DMATxOnlyAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   HAL_UART_AbortTransmitCpltCallback(huart);
UART_DMATxOnlyAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 2879 :   *         HAL_UART_AbortReceive_IT API (Abort only Rx transfer)
UART_DMARxOnlyAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->RxState = HAL_UART_STATE_READY;
UART_DMARxOnlyAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
UART_DMARxOnlyAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   HAL_UART_AbortReceiveCpltCallback(huart);
UART_DMARxOnlyAbortCallback in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
UART_Transmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if (huart->gState == HAL_UART_STATE_BUSY_TX)
UART_Transmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       __HAL_UART_DISABLE_IT(huart, UART_IT_TXE);
UART_Transmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       __HAL_UART_ENABLE_IT(huart, UART_IT_TC);
UART_EndTransmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   __HAL_UART_DISABLE_IT(huart, UART_IT_TC);
UART_EndTransmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   huart->gState = HAL_UART_STATE_READY;
UART_EndTransmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
UART_EndTransmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   HAL_UART_TxCpltCallback(huart);
UART_EndTransmit_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
UART_Receive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :   if (huart->RxState == HAL_UART_STATE_BUSY_RX)
UART_Receive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       __HAL_UART_DISABLE_IT(huart, UART_IT_RXNE);
UART_Receive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       __HAL_UART_DISABLE_IT(huart, UART_IT_PE);
UART_Receive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       __HAL_UART_DISABLE_IT(huart, UART_IT_ERR);
UART_Receive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       huart->RxState = HAL_UART_STATE_READY;
UART_Receive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
UART_Receive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) :       HAL_UART_RxCpltCallback(huart);
UART_Receive_IT in stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
stm32f2xx_hal_uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Src) line 3121 : #endif /* HAL_UART_MODULE_ENABLED */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 3 :   * @file    stm32f2xx_hal_uart.h
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 21 : #ifndef __STM32F2xx_HAL_UART_H
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 22 : #define __STM32F2xx_HAL_UART_H
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 119 :   HAL_UART_STATE_RESET             = 0x00U,    /*!< Peripheral is not yet Initialized
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 121 :   HAL_UART_STATE_READY             = 0x20U,    /*!< Peripheral Initialized and ready for use
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 123 :   HAL_UART_STATE_BUSY              = 0x24U,    /*!< an internal process is ongoing
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 125 :   HAL_UART_STATE_BUSY_TX           = 0x21U,    /*!< Data Transmission process is ongoing
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 127 :   HAL_UART_STATE_BUSY_RX           = 0x22U,    /*!< Data Reception process is ongoing
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 129 :   HAL_UART_STATE_BUSY_TX_RX        = 0x23U,    /*!< Data Transmission and Reception process is ongoing
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 132 :   HAL_UART_STATE_TIMEOUT           = 0xA0U,    /*!< Timeout state
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 134 :   HAL_UART_STATE_ERROR             = 0xE0U     /*!< Error
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 136 : } HAL_UART_StateTypeDef;
__UART_HandleTypeDef in stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) :   __IO HAL_UART_StateTypeDef    gState;           /*!< UART state information related to global Handle management
__UART_HandleTypeDef in stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) :                                                        This parameter can be a value of @ref HAL_UART_StateTypeDef */
__UART_HandleTypeDef in stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) :   __IO HAL_UART_StateTypeDef    RxState;          /*!< UART state information related to Rx operations.
__UART_HandleTypeDef in stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) :                                                        This parameter can be a value of @ref HAL_UART_StateTypeDef */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 174 : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 187 : #endif  /* USE_HAL_UART_REGISTER_CALLBACKS */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 191 : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 197 :   HAL_UART_TX_HALFCOMPLETE_CB_ID         = 0x00U,    /*!< UART Tx Half Complete Callback ID        */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 198 :   HAL_UART_TX_COMPLETE_CB_ID             = 0x01U,    /*!< UART Tx Complete Callback ID             */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 199 :   HAL_UART_RX_HALFCOMPLETE_CB_ID         = 0x02U,    /*!< UART Rx Half Complete Callback ID        */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 200 :   HAL_UART_RX_COMPLETE_CB_ID             = 0x03U,    /*!< UART Rx Complete Callback ID             */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 201 :   HAL_UART_ERROR_CB_ID                   = 0x04U,    /*!< UART Error Callback ID                   */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 202 :   HAL_UART_ABORT_COMPLETE_CB_ID          = 0x05U,    /*!< UART Abort Complete Callback ID          */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 203 :   HAL_UART_ABORT_TRANSMIT_COMPLETE_CB_ID = 0x06U,    /*!< UART Abort Transmit Complete Callback ID */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 204 :   HAL_UART_ABORT_RECEIVE_COMPLETE_CB_ID  = 0x07U,    /*!< UART Abort Receive Complete Callback ID  */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 205 :   HAL_UART_WAKEUP_CB_ID                  = 0x08U,    /*!< UART Wakeup Callback ID                  */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 207 :   HAL_UART_MSPINIT_CB_ID                 = 0x0BU,    /*!< UART MspInit callback ID                 */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 208 :   HAL_UART_MSPDEINIT_CB_ID               = 0x0CU     /*!< UART MspDeInit callback ID               */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 210 : } HAL_UART_CallbackIDTypeDef;
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 217 : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 231 : #define HAL_UART_ERROR_NONE              0x00000000U   /*!< No error            */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 232 : #define HAL_UART_ERROR_PE                0x00000001U   /*!< Parity error        */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 233 : #define HAL_UART_ERROR_NE                0x00000002U   /*!< Noise error         */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 234 : #define HAL_UART_ERROR_FE                0x00000004U   /*!< Frame error         */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 235 : #define HAL_UART_ERROR_ORE               0x00000008U   /*!< Overrun error       */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 236 : #define HAL_UART_ERROR_DMA               0x00000010U   /*!< DMA transfer error  */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 237 : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 238 : #define  HAL_UART_ERROR_INVALID_CALLBACK 0x00000020U   /*!< Invalid Callback error  */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 239 : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 387 : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 388 : #define __HAL_UART_RESET_HANDLE_STATE(__HANDLE__)  do{                                                   \
__HAL_UART_RESET_HANDLE_STATE in stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) :                                                        (__HANDLE__)->gState = HAL_UART_STATE_RESET;      \
__HAL_UART_RESET_HANDLE_STATE in stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) :                                                        (__HANDLE__)->RxState = HAL_UART_STATE_RESET;     \
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 395 : #define __HAL_UART_RESET_HANDLE_STATE(__HANDLE__)  do{                                                   \
__HAL_UART_RESET_HANDLE_STATE in stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) :                                                        (__HANDLE__)->gState = HAL_UART_STATE_RESET;      \
__HAL_UART_RESET_HANDLE_STATE in stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) :                                                        (__HANDLE__)->RxState = HAL_UART_STATE_RESET;     \
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 399 : #endif /*USE_HAL_UART_REGISTER_CALLBACKS */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 406 : #define __HAL_UART_FLUSH_DRREGISTER(__HANDLE__) ((__HANDLE__)->Instance->DR)
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 426 : #define __HAL_UART_GET_FLAG(__HANDLE__, __FLAG__) (((__HANDLE__)->Instance->SR & (__FLAG__)) == (__FLAG__))
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 450 : #define __HAL_UART_CLEAR_FLAG(__HANDLE__, __FLAG__) ((__HANDLE__)->Instance->SR = ~(__FLAG__))
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 458 : #define __HAL_UART_CLEAR_PEFLAG(__HANDLE__)     \
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 472 : #define __HAL_UART_CLEAR_FEFLAG(__HANDLE__) __HAL_UART_CLEAR_PEFLAG(__HANDLE__)
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 480 : #define __HAL_UART_CLEAR_NEFLAG(__HANDLE__) __HAL_UART_CLEAR_PEFLAG(__HANDLE__)
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 488 : #define __HAL_UART_CLEAR_OREFLAG(__HANDLE__) __HAL_UART_CLEAR_PEFLAG(__HANDLE__)
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 496 : #define __HAL_UART_CLEAR_IDLEFLAG(__HANDLE__) __HAL_UART_CLEAR_PEFLAG(__HANDLE__)
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 514 : #define __HAL_UART_ENABLE_IT(__HANDLE__, __INTERRUPT__)   ((((__INTERRUPT__) >> 28U) == UART_CR1_REG_INDEX)? ((__HANDLE__)->Instance->CR1 |= ((__INTERRUPT__) & UART_IT_MASK)): \
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 534 : #define __HAL_UART_DISABLE_IT(__HANDLE__, __INTERRUPT__)  ((((__INTERRUPT__) >> 28U) == UART_CR1_REG_INDEX)? ((__HANDLE__)->Instance->CR1 &= ~((__INTERRUPT__) & UART_IT_MASK)): \
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 553 : #define __HAL_UART_GET_IT_SOURCE(__HANDLE__, __IT__) (((((__IT__) >> 28U) == UART_CR1_REG_INDEX)? (__HANDLE__)->Instance->CR1:(((((uint32_t)(__IT__)) >> 28U) == UART_CR2_REG_INDEX)? \
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 558 :   *         without need to call HAL_UART_Init() function.
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 562 :   *           - UART instance should have already been initialised (through call of HAL_UART_Init() )
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 563 :   *           - macro could only be called when corresponding UART instance is disabled (i.e __HAL_UART_DISABLE(__HANDLE__))
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 564 :   *             and should be followed by an Enable macro (i.e __HAL_UART_ENABLE(__HANDLE__)).
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 570 : #define __HAL_UART_HWCONTROL_CTS_ENABLE(__HANDLE__)        \
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 578 :   *         without need to call HAL_UART_Init() function.
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 582 :   *           - UART instance should have already been initialised (through call of HAL_UART_Init() )
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 583 :   *           - macro could only be called when corresponding UART instance is disabled (i.e __HAL_UART_DISABLE(__HANDLE__))
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 584 :   *             and should be followed by an Enable macro (i.e __HAL_UART_ENABLE(__HANDLE__)).
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 590 : #define __HAL_UART_HWCONTROL_CTS_DISABLE(__HANDLE__)        \
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 598 :   *         without need to call HAL_UART_Init() function.
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 602 :   *           - UART instance should have already been initialised (through call of HAL_UART_Init() )
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 603 :   *           - macro could only be called when corresponding UART instance is disabled (i.e __HAL_UART_DISABLE(__HANDLE__))
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 604 :   *             and should be followed by an Enable macro (i.e __HAL_UART_ENABLE(__HANDLE__)).
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 610 : #define __HAL_UART_HWCONTROL_RTS_ENABLE(__HANDLE__)       \
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 618 :   *         without need to call HAL_UART_Init() function.
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 622 :   *           - UART instance should have already been initialised (through call of HAL_UART_Init() )
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 623 :   *           - macro could only be called when corresponding UART instance is disabled (i.e __HAL_UART_DISABLE(__HANDLE__))
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 624 :   *             and should be followed by an Enable macro (i.e __HAL_UART_ENABLE(__HANDLE__)).
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 630 : #define __HAL_UART_HWCONTROL_RTS_DISABLE(__HANDLE__)       \
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 640 : #define __HAL_UART_ONE_BIT_SAMPLE_ENABLE(__HANDLE__) ((__HANDLE__)->Instance->CR3|= USART_CR3_ONEBIT)
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 646 : #define __HAL_UART_ONE_BIT_SAMPLE_DISABLE(__HANDLE__) ((__HANDLE__)->Instance->CR3 &= (uint16_t)~((uint16_t)USART_CR3_ONEBIT))
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 652 : #define __HAL_UART_ENABLE(__HANDLE__)               ((__HANDLE__)->Instance->CR1 |=  USART_CR1_UE)
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 658 : #define __HAL_UART_DISABLE(__HANDLE__)              ((__HANDLE__)->Instance->CR1 &=  ~USART_CR1_UE)
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 673 : HAL_StatusTypeDef HAL_UART_Init(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 677 : HAL_StatusTypeDef HAL_UART_DeInit(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 678 : void HAL_UART_MspInit(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 679 : void HAL_UART_MspDeInit(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 682 : #if (USE_HAL_UART_REGISTER_CALLBACKS == 1)
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 683 : HAL_StatusTypeDef HAL_UART_RegisterCallback(UART_HandleTypeDef *huart, HAL_UART_CallbackIDTypeDef CallbackID, pUART_CallbackTypeDef pCallback);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 684 : HAL_StatusTypeDef HAL_UART_UnRegisterCallback(UART_HandleTypeDef *huart, HAL_UART_CallbackIDTypeDef CallbackID);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 685 : #endif /* USE_HAL_UART_REGISTER_CALLBACKS */
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 696 : HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 697 : HAL_StatusTypeDef HAL_UART_Receive(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 698 : HAL_StatusTypeDef HAL_UART_Transmit_IT(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 699 : HAL_StatusTypeDef HAL_UART_Receive_IT(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 700 : HAL_StatusTypeDef HAL_UART_Transmit_DMA(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 701 : HAL_StatusTypeDef HAL_UART_Receive_DMA(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 702 : HAL_StatusTypeDef HAL_UART_DMAPause(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 703 : HAL_StatusTypeDef HAL_UART_DMAResume(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 704 : HAL_StatusTypeDef HAL_UART_DMAStop(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 706 : HAL_StatusTypeDef HAL_UART_Abort(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 707 : HAL_StatusTypeDef HAL_UART_AbortTransmit(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 708 : HAL_StatusTypeDef HAL_UART_AbortReceive(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 709 : HAL_StatusTypeDef HAL_UART_Abort_IT(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 710 : HAL_StatusTypeDef HAL_UART_AbortTransmit_IT(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 711 : HAL_StatusTypeDef HAL_UART_AbortReceive_IT(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 713 : void HAL_UART_IRQHandler(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 714 : void HAL_UART_TxCpltCallback(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 715 : void HAL_UART_TxHalfCpltCallback(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 716 : void HAL_UART_RxCpltCallback(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 717 : void HAL_UART_RxHalfCpltCallback(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 718 : void HAL_UART_ErrorCallback(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 719 : void HAL_UART_AbortCpltCallback(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 720 : void HAL_UART_AbortTransmitCpltCallback(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 721 : void HAL_UART_AbortReceiveCpltCallback(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 744 : HAL_UART_StateTypeDef HAL_UART_GetState(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 745 : uint32_t              HAL_UART_GetError(UART_HandleTypeDef *huart);
stm32f2xx_hal_uart.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc) line 844 : #endif /* __STM32F2xx_HAL_UART_H */
USART1_IRQHandler in stm32f2xx_it.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :   HAL_UART_IRQHandler(&huart1);
USART3_IRQHandler in stm32f2xx_it.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :   if ((__HAL_UART_GET_FLAG(&huart3, UART_FLAG_RXNE) != RESET))
USART3_IRQHandler in stm32f2xx_it.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :    __HAL_UART_CLEAR_PEFLAG(&huart3); /* clear event flag */
USART3_IRQHandler in stm32f2xx_it.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :   HAL_UART_IRQHandler(&huart3);
stm32_hal_legacy.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc\Legacy) line 1146 : /** @defgroup HAL_UART_Aliased_Defines HAL UART Aliased Defines maintained for legacy purpose
stm32_hal_legacy.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc\Legacy) line 1154 : #define __HAL_UART_ONEBIT_ENABLE        __HAL_UART_ONE_BIT_SAMPLE_ENABLE
stm32_hal_legacy.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc\Legacy) line 1155 : #define __HAL_UART_ONEBIT_DISABLE       __HAL_UART_ONE_BIT_SAMPLE_DISABLE
stm32_hal_legacy.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc\Legacy) line 1524 : /** @defgroup HAL_UART_Aliased_Functions HAL UART Aliased Functions maintained for legacy purpose
stm32_hal_legacy.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc\Legacy) line 1527 : #define HAL_UART_WakeupCallback HAL_UARTEx_WakeupCallback
stm32_hal_legacy.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc\Legacy) line 3430 : /** @defgroup HAL_UART_Aliased_Macros HAL UART Aliased Macros maintained for legacy purpose
stm32_hal_legacy.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc\Legacy) line 3434 : #define __HAL_UART_GETCLOCKSOURCE       UART_GETCLOCKSOURCE
stm32_hal_legacy.h (D:\workspace\STM32F207_ChannelCtrlProject\Drivers\STM32F2xx_HAL_Driver\Inc\Legacy) line 3435 : #define __HAL_UART_MASK_COMPUTATION     UART_MASK_COMPUTATION
Uart1_Data_Send in uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     HAL_UART_Transmit_DMA(&huart1, data,size);
Uart3_Data_Send in uart.c (D:\workspace\STM32F207_ChannelCtrlProject\Src) :     HAL_UART_Transmit_DMA(&huart3, data,size);
